Sending a MBF to the Radiometer

After a batch is created it can be sent to the radiometer (assuming the host is connected to it). Alternatively, a single MDF can be sent.
This is done with the Send Measurement Batch File to Radiometer menu.
By entering this menu the host determines the current radiometer configuration and analyzes the available frequency channel list and other capabilities of the connected radiometer hardware.
When an MBF is loaded (Load Batch File), its contents and repetition factor are displayed. In addition, some pre-checks are performed, e.g. correct radiometer configuration, frequency list consistency, etc. A variety of other checks ensure that no erroneous command data is sent.
When the consistency check of a MDF is finished, the test result is displayed in the Check List. The batch can only be sent to the radiometer if all consistency checks have finished with the status OK. Then the MBF is transmitted with Send Batch to Radiometer.